상품상세설명 추가파일 #1

What we can provide you

● Shipbuilding Design & Offshore Business & Marine Engineering

Outline Spec,  Preliminary Cabin Layout , Cost Estimation, etc.

● Basic(FEED/EPC) and Detail Design

(All kinds of Drawings for Classification & Approval)

Develop Cabin Plan, 3D Perspective Design, Related to detail design etc.

All kinds of Basic and Detail Drawings including Diagrams and other Technical

Documentations for Owners/Class Approval

● Production Design (by 3D Modeling)

Hull Production Drawings

(for Cutting, Forming, Assembly, Remarking, Template, etc.)

Hull Piping, Engine Room Piping

Hull Outfitting, Engine Room Outfitting

Accommodation Outfitting

Electrical / Electronic Equipment & Outfitting

Material & Production related Information

(BOM, PML, Control of Scrap Ratio & Leftover Steel Plates etc.)

● Process Review

Vision & Strategy

Selection of Vendor

Management of Engineering

Preparation of related to document such as RFQ,TBE & POS

Quality Management

Performance Evaluation

Sales & Marketing Strategy

● What is the TLQ?

It means the abbreviation of "Temporary Living Quarter"

In that case Offshore work is finished in incomplete condition,

it is used for workers commonly during boarding as temporary

residence container.

Or when the vessel shuts down in offshore work, it is used as living space for

temporary workers.

◎ MODULE CABIN SPECIFICATION(Include Small Recreation Area-Chair And Table)

Dimension : 8'X20'(2,438mmX6,096mm), 8'X40'(2,438mmX12,192mm) standard size for

easy transportation.

A-60 class fire rating roof, bulkhead and deck.

A-60 class fire rating door with weather tight type with self closing device.

Vinyl sheet on floor covering.

Heating, ventilation and air conditioning.

Unit toilet system.

Connection for main electric power.

Connection for cold water supply.

2 tier berth with mattress include curtain.

Cloth locker for each person.

Writing desk, book rack and chair.

Coat hook & Hat hook.

◎ MODULE OFFICE SPECIFICATION

Dimension : 8'X20'(2,438mmX6,096mm) standard size for easy transportation.

A-60 class fire rating roof, bulkhead and deck.

A-60 class fire rating door with weather tight type with self closing device.

Vinyl sheet on floor covering.

Heating, ventilation and air conditioning.

Connection for main electric power.

Window with curtain, curtain box.

4 writing desk(include side desk) with chair.

2 fitting cabinet.

1 fitting drawer.

Accessory.

◎ MODULE MESSROOM SPECIFICATION

Dimension : 8'X20'(2,438mmX6,096mm) standard size for easy transportation.

A-60 class fire rating roof, bulkhead and deck.

A-60 class fire rating door with weather tight type with self closing device.

Vinyl sheet on floor covering.

Heating, ventilation and air conditioning.

Connection for main electric power.

Window with curtain, curtain box.

3 mess table with 12 chair.

1 fitting sink and bowl.

1 fitting white board, bulletin board.

Accessory.

◎ MODULE TOILET SPECIFICATION

Dimension : 8'X20'(2,438mmX6,096mm) standard size for easy transportation.

A-60 class fire rating roof, bulkhead and deck.

A-60 class fire rating door with weather tight type with self closing device.

Cream tile on cement mortar.

Heating, ventilation and air conditioning.

Connection for main electric power.

Connection for cold water supply.

Hot water boiler to be provided.

Access floor area for plumbing to be provided.

Coat hook & hat hook.

Mirror.

◎ MODULE ELECTRIC HOUSE SPECIFICATION

Dimension : 8'X40'(2,438mmX12,192mm) standard size for easy transportation.

A-60 class fire rating roof, bulkhead and deck.

A-60 class fire rating door with weather tight type with self closing device.

Vinyl sheet on floor covering.

Heating, ventilation and air conditioning.

Connection for main electric power.

2 writing desk(include side book rack) with chair.

2 fitting cabinet.

1 fitting drawer.

1 fitting white board, bulletin board

Accessory.

◎ MODULE CONTAINER FOR PAINT LOCKER, TOOL LOCKER, STORE ETC. SPECIFICATION

Dimension : 8'X40'(2,438mmX12,192mm) standard size for easy transportation.

A-60 class fire rating roof, bulkhead and deck.

A-60 class fire rating door with weather tight type with self closing device.

SHELF

● FIRE DAMPER A-0, A-60 CLASS SPECIFICATION

A-60 Pneumatic type Fire Damper

A-0, A-60 Electric type Fire Damper

Tested and approved "A-0, A-60" class divisions according IMO754(18). Certified by

major Class, "MED", "C.E" notified by DNV, ABS.

Operating and Control Method : Automatic & Pneumatic Electrically

Adjusted dimension and special type Fire Damper shall be provided customer

requirement.

● FIRE SHUTTER

Electric and manual Roll-Up Fire Shutter(door) is a robust safety device.

It's designed to prevent fire & gas spreading between galley and mess room or A-0

class regulation required area.

Tested approved "A-0" class divisions according IMO754(18).

Certified by major Class, "MED", "CE" notified by DNV and type  approved by ABS.

● GALLEY EQUIPMENT

◎ COOKING RANGE

◎ ELECTRIC KETTLE, ELECTRIC SOUP BOILER

◎ ELECTRIC FRYING PAN, ELECTRIC GRIDDLE, DEEP FAT FRYER

◎ ELECTRIC BAIN MARIE

◎ ELECTRIC BAKING OVEN, CONVECTION COMBI-OVEN,

◎ REFRIGERATOR/FREEZER, PREPARATION EQUIPMENTS, ETC

One is modular system and the other is un-modular system. All of catering

furniture is divided into NSF(National Sanitation Foundation, USA) model and

non-NSF model. There are differences in thickness of stainless steel sheet,

● GALLEY HOOD SPECIFICATION

Supply Air(Duct) : Ventilation bringing fresh air from outside.

Exhaust Air(Duct) : Exhaust Duct emitting polluted air inside.

● PANELLING SYSTEM

◎ WALL PANEL

◎ CEILING PANEL

● DOOR SYSTEM

Tested and approved "B-0, -15, A-0, A-60" class divisions according IMO754(18).       Certified by major Class, "MED", "C.E" notified by DNV, ABS.

◎ B-CLASS DOOR incl. HIGH NOISE REDUCTION DOOR

◎ A-CLASS DOOR

◎ SLIDING DOOR

● UNIT TOILET SYSTEM

◎ SHOWER TOILET

◎ BATH TOILET

● COLD PROVISION CHAMBER & RAISED FLOOR SYSTEM

◎ REACH in SYSTEM

◎ MODULAR WALK-in COLD CHAMBER

● MARINE ELEVATOR SYSTEM

◎ SERVICE ELEVATOR

◎ CREW ELEVATOR

◎ PASSENGER ELEVATOR

◎ DUMBWAITER

● DRYING SYSTEM MARITIME

◎ WALL-MOUNTED DRYING SYSTEM

◎ CABINET DRYING SYSTEM

◎ CONTAINER DRYING SYSTEM

◎ MOBILE/ FREE STANDING SYSTEM

● STAINER SYSTEM

◎ BALLAST WATER AUTO FILTER

◎ MAIN SEA WATER AUTO FILTER

◎ HEAVY FUEL OIL AUTO FILTER

● WINDOW WIPER & CLEAR VIEW SCREEN

● FURNITURE

◎ WOODEN FURNITURE

◎ STEEL FURNITURE

● DECK COVERING SYSTEM

◎ LATEX TYPE DECK COMPOSITION

◎ SELF LEVELLING TYPE DECK COMPOSITION

◎ A-60 DECK COMPOSITION

◎ SOUND REDUCTION

◎ EPOXY SELF LEVELLING

◎ EPOXY TILE ADHESIVE

◎ EPOXY GROUTING BETWEEN TILES

● BOILER SYSTEM